Adding Custom IP to the System

Introduction

This lab guides you through the process of creating and adding a custom peripheral to a processor system by using the Vivado IP Packager. You will create an AXI4Lite interface peripheral.

# Objectives

After completing this lab, you will be able to:

* Use the IP Packager feature of Vivado to create a custom peripheral
* Modify the functionality of the IP
* Add the custom peripheral to your design
* Add pin location constraints
* Add block memory to the system

Procedure

This lab is separated into steps that consist of general overview statements that provide information on the detailed instructions that follow. Follow these detailed instructions to progress through the lab.

This lab comprises 4 primary steps: You will use a peripheral template to create a peripheral, Package the IP using IP Packager, import, add and connect the IP in the design, and add the Block RAM (BRAM) Memory.

Design Description

You will extend the Lab 2 hardware design by creating and adding an AXI peripheral (refer to LED\_IP in **Figure 1**) to the system, and connecting it to the LEDs on the ZYBO board.You will use the IP Packager to generate the custom IP. Next, you will connect the peripheral to the system and add pin location constraints to connect the LED display controller peripheral to the on-board LED display. Finally, you will add BRAM Controller and BRAM before generating the bitstream.




Figure 1. Design Updated from Previous Lab

General Flow for this Lab

Step 1: Create Custom IP using

Peripheral Template

Step 2: Package Peripheral using IP Packager

Step 3:

Set the Project Settings

Step 4:

Add the IP. BRAM, and Constraints

1. Create a Custom IP using the Create and Package IP Wizard Step
   1. Use the provided axi\_lite slave peripheral template and the custom IP source code to create a custom IP.
      1. Open Vivado by selecting **Start > All Programs > Xilinx Design Tools > Vivado 2013.4 > Vivado 2013.4**
      2. Click **Manage IP** and select *New IP Location* and click **Next** in the *New IP Location* window
      3. Select **Verilog** as the *Target Language*, **Mixed** as the *Simulator language*, and for *IP location*, type *C:\xup\embedded\labs\led\_ip* and click **Finish** (leave other settings as defaults)




Figure 2. New IP Location form

A Virtex 7 part is chosen for this project, but later compatibility for other devices will be added to the packaged IP later.

* + 1. Click **OK** to create the *led\_ip* directory.
  1. Run the Create and Package IP Wizard
     1. Select *Tools > Create and Package IP*
     2. In the window, click **Next**
     3. Select *Create new AXI4 peripheral*, specify the *IP Definition location* as *C:/xup/embedded/labs/led\_ip* and click **Next**
     4. Fill in the details for the IP

*Name:* **led\_ip**

*Display Name*: **led\_ip\_v1\_0**

(Fill in a description, Vendor Name, and URL)




Figure 3. Updating Peripheral Details form

* + 1. Click **Next**
    2. Change the Name of the interface to **S\_AXI**
    3. Leave the other settings as default and click **Next** (Lite interface, Slave mode, Data Width 32, Registers 4)




Figure 4. Naming the AXI interface

* + 1. Select *Generate Drivers* and click **Next**
    2. Select *Add IP to Catalog and open IP in editing session* selected and click **Finish**
    3. In the sources panel, double-click the **led\_ip\_v1\_0.v** file and scroll down to line 15 where users port definition space is provided.
    4. Add the line:

**output wire [3:0] LED,**

(Notice the extra comma needed at the end of line)




Figure 5. Adding users port definition

* + 1. Insert the following at line ~48:

**. LED(LED),**




Figure 6. Adding port connection with a lower-level module

* + 1. Save the file by selecting **File > Save File**
    2. Expand *led\_ip\_v1\_0* in the sources view if necessary, and open **led\_ip\_v1\_0\_S\_AXI.v**
    3. Add the LED port to this file too, at line 15




Figure 7. Declaring users port in the lower-level module

* + 1. Scroll down to ~line 397 and insert the following code to instantiate the user logic for the LED IP

(This code can be typed directly, or copied from the user\_logic\_instantiation.txt file in the lab3 source folder.)




Figure 8. Instantiating lower-level user module

Check all the signals that are being connected and where they originate.

* + 1. Save the file by selecting **File > Save File**
    2. Click on the *Add Sources* in the Flow Navigator pane, select *Add or Create Design Sources*, browse to *c:\xup\embedded\sources\lab3*, select the **lab3\_user\_logic.v** file and click **OK,** and then click **Finish** to add the file.

Check the contents of this file to understand the logic that is being implemented. Notice the formed hierarchy.

* + 1. Click **Run Synthesis** and *Save* if prompted*.* (This is to check the design synthesizes correctly before packaging the IP.
    2. **Check the *Messages* tab for any errors and correct if necessary before moving to the next step**

When Synthesis completes successfully, click **Cancel**.

It is important that all source files that the IP will use be located under the IP project.

* 1. Update the IP project with the necessary source files in the appropriate directory
     1. Expand the source hierarchy, if needed, and select lab3\_user\_logic entry.
     2. Right-click and select **Remove File from the Project**.
     3. Click OK to remove the file.

Similarly, remove all the files which were added from outside the project directory. In this lab, you don’t have more files to be removed.

* + 1. Using Windows Explorer, copy the *lab3\_user\_logic.v* file from the **c:\xup\embedded\sources\lab3** directory and paste it in the current IP project directory at **c:\xup\embedded\labs\led\_ip\led\_ip\_1.0\hdl** directory.
    2. Click on the *Add Sources* in the Flow Navigator pane, select *Add or Create Design Sources*, browse to *c:\xup\embedded\labs\led\_ip\led\_ip\_1.0\hdl*, select the **lab3\_user\_logic.v** file and click **OK,** and then click **Finish** to add the file.

Make sure that you select the file from the IP project directory and not the sources\lab3 directory.

* 1. Package the IP
     1. Click on the **Package IP – led\_ip** tab
     2. For the IP to appear in the IP catalog in particular categories, the IP must be configured to be part of those categories. To change which categories the IP will appear in the IP catalog click the browse box on the *Categories* line. This opens the Choose IP Categories window
     3. For the exercise purpose, uncheck the **AXI Peripheral** box and check the **Basic Elements** and click **OK**.




Figure 9. Specify the category for IP Packager IP

* + 1. Select **IP Compatibility**. This shows the different Xilinx FPGA Families that the IP supports. The value is inherited from the device selected for the project.
    2. Right click in the *Family Support table* and select **Add Family…** from the menu.
    3. Select the **Zynq** family as we will be using this IP on the ZYBO board, and click **OK**.
    4. You can also customize the address space and add memory address space using the **IP Addressing and Memory** category. We won’t make any changes.
    5. Click on **IP File Groups** *and click Merge changes from IP File Groups Wizard*




Figure 10. Updating the file group

This is to update the IP Packager with the changes that were made to the IP and the *lab3\_user\_logic.v* file that was added to the project.

* + 1. Do the same for IP Customization Parameters (*Merge changes from IP Customization Parameters Wizard*)

Notice that the *IP Ports* view now shows the user created *LED* port




Figure 11. User port imported

* + 1. Select *Review and Package*, and notice the path where the IP will be created.




Figure 12. IP location

* + 1. Click **Re-Package IP**

You will see a warning message indicating that the led\_ip directory is already in the project. Click OK to ignore it.

* + 1. In the Vivado window click **File > Close Project**

1. Modify the Project Settings Step 3
   1. Open the previous project, or use the lab2 project from the labsolution directory, and save the project as lab3. Set Project Settings to point to the created IP repository.
      1. Start the Vivado if necessary and open either the lab2 project you created in the previous lab or the lab2 project in the labsolution directory
      2. Select **File > Save Project As …** to open the *Save Project As* dialog box. Enter **lab3** as the project name. Make sure that the *Create Project Subdirectory* option is checked, the project directory path is c:\xup\embedded\labs\ and click **OK**.

This will create the lab3 directory and save the project and associated directory with lab3 name.

* + 1. Click **Project Settings** in the *Flow Navigator* pane.
    2. Select **IP** in the left pane of the *Project Settings* form.
    3. Click on the **Add Repository…** button, browse to **c:\xup\embedded\labs\led\_ip** and click **Select**.

The led\_ip\_v1\_0 IP will appear the **IP in the Selected Repository** window.




Figure 13. Specify IP Repository

* + 1. Click **OK**.

1. Add the Custom IP, BRAM, and the Constraints Step 4
   1. Add led\_ip to the design and connect to the AXI4Lite interconnect in the IPI. Make internal and external port connections. Establish the LED port as external FPGA pins.
      1. Click **Open Block Design** under **IP Integrator** in the Flow Navigator pane, and select **system.bd** to open IP Integrator
      2. Click the Add IP icon  and search for **led\_ip\_v1\_0** in the catalog by typing “led” in the search field.




Figure 12. Searching for led\_ip in the IP Catalog

* + 1. Double-click **led\_ip\_v1\_0** to add the core to the design.
    2. Select the IP in the block diagram and change the instance name to **led\_ip** in the properties view.
    3. Click on **Run Connection Automation**, select **/led\_ip/S\_AXI** and click **OK** to automatically make the connection from the AXI Interconnect to the IP.
    4. Click the regenerate button () to redraw the diagram.




Figure 13. LED IP Block added and connected

* + 1. Select the *LED[3:0]* port on the led\_ip instance (by clicking on its pin), right-click and select **Make External**.




Figure 14. LED external port added and connected

* + 1. Select the **Address Editor** tab and verify that an address has been assigned to *led\_ip*.




Figure 15. Address assigned for led\_ip

* 1. Add BRAM to the design
     1. In the Block Diagram, click the Add IP icon  and search for BRAM and add one instance of the **AXI BRAM Controller**
     2. Run *Connection Automation* on **axi\_bram\_ctrl\_0/S\_AXI** and click **OK** when prompted to connect it to the **M\_AXI\_GP0 Master.**
     3. Double click on the block to customize it and change the number of BRAM interfaces to 1 and click **OK**.

Notice that the AXI Protocol being used is AXI4 instead of AXI4Lite since BRAM can provide higher bandwidth and the controller can support burst transactions.




Figure 16. Customize BRAM controller

* + 1. Run *Connection Automation* to add and connect a **Block Memory Generator** (This could be added manually)
    2. Validate the design to ensure there are no errors, and click the regenerate button () to redraw the diagram.

The design should look similar to the figure below.




Figure 17. Completed Block Diagram

* + 1. In the Address editor, increase the Range of the **axi­\_bram\_ctrl\_0** to **8K**




Figure 20. Adjusting memory size

* + 1. Press **F6** to validate the design one last time.
  1. Update the top-level wrapper and add the provided lab3\_system.xdc constraints file.
     1. In the *sources* view, right-click on the block diagram file, **system.bd**, and select **Create HDL Wrapper** to update the HDL wrapper file, and when prompted, select *Let Vivado Manage Wrapper* *and auto-update* and click **OK**

The system\_wrapper.vhd file will be updated to include the new IP and ports. Double-click on the system-wrapper content to verify that LED port has been added.

* + 1. Click **Add Sources** in the *Flow Navigator* pane, select **Add or Create Constraints**, and click **Next**.
    2. Click the **Add Files** button, browse to the **c:\xup\embedded\sources\lab3** folder, select **lab3\_system.xdc**
    3. Click **Finish** to add the file.
    4. Expand Constraints folder in the *Sources* pane, and double-click **lab3\_system.xdc** file entry to see its content. This file contains the pin locations and IO standards for the LEDs on the ZYBO board. This information can usually be found in the manufacturer’s datasheet for the board.
    5. Click on the **Generate Block Design > system.bd** in the Flow Navigator, to generate the output products of various IPs added to the project.
    6. Select **File > Close Project** to close the project as we will implement the design in the next lab.
    7. Click **Save,** and **OK** to save the design and close the project.

Conclusion

Vivado IP packager was used to import a custom IP block into the IP library. The IP block was then added to the system. Connection automation was run where available to speed up the design of the system by allowing Vivado to automatically make connections between IP. An additional BRAM was added to the design. Finally, pin location constraints were added to the design.